Burn the Raspi x64 verison to a Raspi

Using Raspi Imager

Completed

Open the /boot drive

Edit the config.txt file

Add the following lines to the end of the file

avoid\_warnings=2

max\_usb\_current=1

program\_usb\_boot\_mode=1

arm\_freq=1200

Connect the USB to the Raspi and reboot

The green LED will start blinking after 10seconds.

Root Partition will be resized and the node will again reboot.

wAit for the desktop to load.

It will take 3minutes